Read Before Installing hp DECforms for OpenVMS Systems, Version 3.3

January 2003

Whether you are a new or existing HP DECforms customer, please take time to read the following information about your product.

1 KIT NAME:

FORMSAN033 or FORMSAAN033 (Full Development) FORMSRTAN033 or FORMSRTAAN033 (Run-time)

2 OLD PRODUCT:

DECforms V3.2

3 NEW PRODUCT:

DECforms V3.3

APPROXIMATE BLOCK SIZE: VAX:

Full Development (FORMSAN033) - 67,700 blocks Run-time (FORMSRTAN033) - 6,200 blocks

Alpha:

Full Development (FORMSAAN033) - 78,900 blocks Run-time (FORMSRTAAN033) - 10,400 blocks

DECforms Asian V3.3 Kit Description This kit updates DECforms V3.2.

Installation Overview This kit installation will perform a complete replacement of all existing DECforms components.

To install V3.3 invoke the VMSINSTALL command procedure, as described in the OpenVMS System Manager’s Manual, and follow the instructions in the DECforms Installation Guide for OpenVMS Systems.

NOTE During installation of the V3.3 Asian kit, the release date displays as 2000 rather than 2003. This has no effect on the installation.

© 2003 Hewlett-Packard Development, L.P.